fenugrec 2024
https://www.qcte.ca/testeq/e440x_sa/

Replacement board for 1GC1-4210 divider MMIC.
Uses 2 HMC862 dividers plus decoupling caps.

I recommend panelizing a few copies of this manually, to ensure a clean routing pass on the sides with the castellations.
Otherwise OSHpark may put mousebites there, requiring some extra sanding to get the shape right.
Note that this design pushes the limits of OSHpark design limits, and they may refuse (or fail) to manufacture it.